**Logo

Description automatically generated with medium confidenceSCHEDULE B – FORM OF QUOTATION**

**RFQ Title: Supply and Delivery of One or More Small Double Drum Asphalt Roller**

**RFQ No.: 1220-040-2023-041**

**CONTRACTOR**

**Legal Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Contact Person and Title:**

**Business Address:**

**Business Telephone:**

**Business Fax:**

**Business E-Mail Address:**

TO:

**CITY OF SURREY**

City Representative: Sunny Kaila, Manager, Procurement Services

Email: [purchasing@surrey.ca](mailto:purchasing@surrey.ca)

1. If this offer is accepted by the City, such offer and acceptance will create a contract as described in:

(a) the RFQ;

(b) the specifications of Goods set out above and in Schedule A;

(c) the General Terms and Conditions; and

(d) this Quotation; and

(e) other terms, if any, that are agreed to by the parties in writing.

2. Capitalized terms used and not defined in this Quotation will have the meanings given to them in the RFQ. Except as specifically modified by this Quotation, all terms, conditions, representations, warranties and covenants as set out in the RFQ will remain in full force and effect.

3. I/We have reviewed the RFQ Attachment 1 – Quotation Agreement - Goods. If requested by the City, I/we would be prepared to enter into that Agreement, amended by the following departures (list, if any):

**Section Requested Departure(s) / Alternative(s)**

**Please State Reason For Departure(s):**

**Changes and Additions to Specifications:**

4. In addition to the warranties provided in Attachment 1 – Quotation Agreement - Goods, this Quotation includes the following warranties:

5. I/We have reviewed the RFQ Attachment 1 – Quotation Agreement - Goods, Schedule A – Specifications of Goods. If requested by the City, I/we would be prepared to meet those requirements, amended by the following departures (list, if any):

**Section Requested Departure(s) / Alternative(s) / Additions**

**Please State Reason For Departure(s):**

**Fees and Payments**

6. The Contractor offers to supply to the City of Surrey the Goods for the prices plus applicable taxes as follows:

In accordance with the Agreement, which terms and conditions I/we have carefully examined and agree to, the undersigned hereby submits a firm Quotation for the supply and delivery of the Good in accordance with the Specifications for the price(s) as listed below, delivered F.O.B. Freight Prepaid, City of Surrey, Fleet/Service Centre, Central Operations Works Yard, 6651 – 148th Street, Surrey, B.C. V3S 3C7, CANADA.

The following price(s) include and covers all duties, taxes, handling and transportation charges, and all other charges incidental to and forming part of this Quotation. The Contractor shall be responsible for customs clearance and payment of any duties and/or taxes owing at the time of importation into CANADA, as applicable.

**DOUBLE DRUM ASPHALT ROLLER**

Year, Make & Model: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

All costs to meet the preferred technical specifications should be included in the following delivered prices.

|  |  |  |  |
| --- | --- | --- | --- |
|  | **“Without Trade/s”** |  |  |

|  |  |  |
| --- | --- | --- |
| ROLLER PRICE: |  | $\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| ENVIRONMENTAL LEVIES:  BATTERY: |  | $\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| ANY OTHER LEVIES OR FEES: |  | $\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
|  | SUB-TOTAL: | $\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| GST 5%  H | | $\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| PST 7% | | $\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| **TOTAL QUOTATION PRICE:** | | **$\_\_\_\_\_\_\_\_\_\_\_\_\_\_** |

*Pricing is firm until (state date): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*ALL PRICING IN CANADIAN DOLLARS*

**Payment Terms:**

A cash discount of \_\_\_\_\_\_\_\_ % will be allowed if the invoices are paid within \_\_\_\_\_\_\_ days, or the \_\_\_\_ day of the month following, or net 30 days, on a best effort basis.

**The completed unit should be delivered within \_\_\_\_\_\_\_ days after receipt of purchase order.**

Complete Vehicle: State Warranty (no less than one (1) year)

Extended Warranty Options:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Warranty repairs shall be performed at \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Please complete if applicable: British Columbia Certified

The Contractor should complete and submit with their Quotation the Schedule B-1 Preferred Technical Specifications Response Form. Attach any additional specifications for the Goods, any optional accessories and any substitutions for the Goods (if substitutions are permitted or applicable).

Note: Contractors are directed to list complete manufacturers’ details of model proposed in the right-most column of Schedule B-1

7. I/We the undersigned duly authorized representatives of the Contractor, having received and carefully reviewed the RFQ including without limitation the draft Agreement submit this Quotation in response to the RFQ.

**This Quotation** is offered by the Contractor this \_\_\_\_\_\_\_ day of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, 202\_.

**CONTRACTOR**

I/We have the authority to bind the Contractor.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Full Legal Name of Contractor)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Signature of Authorized Signatory)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Print Name and Position of Authorized Signatory)

**SCHEDULE B-1 – PREFERRED TECHNICAL SPECIFICATIONS RESPONSE FORM**

**PROJECT TITLE: Supply and Delivery of One or More Small Double Drum Asphalt Roller(s)**

**PREFERRED SPECIFICATIONS**

The specification herein states the preferred requirements of the City of Surrey. All Quotations shall be regular in every respect. Unauthorized conditions, limitations, or provisions may be cause for rejection. The City of Surrey will consider as "irregular" or "non-responsive" any Quotation not prepared and submitted in accordance with the RFQ document and specification, or any Quotation lacking sufficient technical literature to enable the City to make a reasonable determination of compliance to the specification.

It shall be the Contractor's responsibility to carefully examine each item of the specification. Failure to offer a completed Quotation or failure to respond to each section of the technical specification may cause the Quotation to be rejected without review as "non-responsive". All variances, exceptions and/or deviations shall be fully described in the appropriate section.

Note: Contractors are directed to list complete manufacturers’ details of model proposed in the right-side column under manufacturers’ specifications.

| **Preferred** **Technical** **Specifications** | **Yes**  **(Circle)** | **No**  **(Circle)** | **Manufacturers’ Specifications of Equipment Offered. Contractor to indicate compliance or deviation with specifications below.** |
| --- | --- | --- | --- |
| 1. **MAKE, MODEL** | | | |
| 1. Make, Model | Y | N |  |
| 1. Model Year | Y | N |  |
| 1. Static weight, no less than 1,700 kgs and no more than 1,850 kgs | Y | N |  |
| 1. **ENGINE** | | | |
| 1. Engine – diesel to meet or exceed EPA Tier 4 final or EU stage V | Y | N |  |
| 1. Engine power approx. 24 hp | Y | N |  |
| 1. Factory-fill long life coolant engine coolant shall be rated to -30 degrees (-30C) | Y | N |  |
| 1. Air cleaner, dual dry element type | Y | N |  |
| 1. **FRAME & DIMESIONS** | | | |
| 1. Overall length approx. 2,050 mm | Y | N |  |
| 1. Overall width approx. 1,010 mm | Y | N |  |
| 1. Drum width shall be 900 mm | Y | N |  |
| 1. Inside turning radius approx. 1,950 mm | Y | N |  |
| 1. Outside turning radius approx. 2,850 mm | Y | N |  |
| 1. Wheelbase approx. 1,375 mm | Y | N |  |
| 1. Curb clearance approx. 400 mm | Y | N |  |
| 1. Articulation angle approx. 32 degrees | Y | N |  |
| 1. Oscillation angle approx. 8 degrees | Y | N |  |
| 1. ROPS frame shall be a folding type | Y | N |  |
| 1. Machine to be supplied with tie down and lift points | Y | N |  |
| 1. Fuel tank capacity – 30 litres |  |  |  |
| 1. **OPERATOR ENVIRONMENT** | | | |
| 1. Operators seat shall have adjustable suspension and operator presence switch | Y | N |  |
| 1. Machine will have a 75 mm wide retractable seat belt as standard | Y | N |  |
| 1. A canopy (weather shield) shall be attached to the ROPS frame, after market option is acceptable | Y | N |  |
| 1. The operator console will come with, emergency stop, rocker switches for controlling machine functions, and warning indicator lights | Y | N |  |
| 1. Two 12 volt power outlets | Y | N |  |
| 1. Horn control | Y | N |  |
| 1. A backup alarm shall be provided | Y | N |  |
| 1. **COMPACTION** | | | |
| 1. Both drums will have folding scrapers | Y | N |  |
| 1. The operator can select the vibration, front, rear or both | Y | N |  |
| 1. Vibration frequency will be approx. 57 Hz | Y | N |  |
| 1. Amplitude will be approx. 0.50mm | Y | N |  |
| 1. Centrifugal force approx. 13.6kN | Y | N |  |
| 1. Water spray tank capacity approx. 145 litres | Y | N |  |
| 1. There will be a pressurized spray system for each drum, with triple filtration and cleanable filters/screens | Y | N |  |
| 1. **HYDRAULICS** | | | |
| 1. Hydraulic system will include variable displacement pump(s), radial constant displacement pumps, and a pump for steering | Y | N |  |
| 1. Service brake will be hydrostatic and work with forward and reverse lever | Y | N |  |
| 1. Parking and emergency brake, failsafe brake on both drums | Y | N |  |
| 1. Travel speed F&R approx. 9 kph | Y | N |  |
| 1. **ELECTRICAL** | | | |
| 1. 12-volt system | Y | N |  |
| 1. Battery capacity 650 CCA | Y | N |  |
| 1. Alternator – 40Amp | Y | N |  |
| 1. Work lights front and rear, with light guards | Y | N |  |
| 1. Rotating amber beacon light to be mounted ROPS frame | Y | N |  |
| 1. **MISCELLANEOUS** | | | |
| 1. Owner manuals, including suggested maintenance intervals | Y | N |  |
| 1. Provide warranty details – minimum of 12 months, provide any extended warranty options.   • Provide Operators Manuals / Service Manuals  • 1 – Service manual or CD c/w software   * A build sheet shall be provided detailing (but not limited to the following): * Serial No. * Engine details including serial number * Hydraulic pumps and motors details, including serial numbers * Oil types and quantities for all components * Engine belts details * Filter list for all components * Battery details | Y | N |  |
| 1. Operator training/familiarization will be provided at no cost to the City | Y | N |  |
| 1. The contractor should deliver the vehicle registered, insured, and plated as per the City’s insurance requirements through the City’s insurance broker. | Y | N |  |

**[END OF PAGE]**