Logo

Description automatically generated with medium confidence

SCHEDULE B - QUOTATION

**RFQ Title: Supply and Delivery of One – 1 Ton Van for Mechanics**

**RFQ No.: 1220-040-2024-084**

**CONTRACTOR**

**Legal Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Contact Person and Title:**

**Business Address:**

**Business Telephone:**

**Business Fax:**

**Business E-Mail Address:**

TO:

**CITY OF SURREY**

City Representative: Sunny Kaila, Manager, Procurement Services

Email: [purchasing@surrey.ca](mailto:purchasing@surrey.ca)

1. If this offer is accepted by the City, such offer and acceptance will create a contract as described in:

(a) the RFQ;

(b) the specifications of Goods set out above and in Schedule A;

(c) the General Terms and Conditions; and

(d) this Quotation; and

(e) other terms, if any, that are agreed to by the parties in writing.

2. Capitalized terms used and not defined in this Quotation will have the meanings given to them in the RFQ. Except as specifically modified by this Quotation, all terms, conditions, representations, warranties and covenants as set out in the RFQ will remain in full force and effect.

3. I/We have reviewed the RFQ Attachment 1 – Quotation Agreement - Goods. If requested by the City, I/we would be prepared to enter into that Agreement, amended by the following departures (list, if any):

**Section Requested Departure(s) / Alternative(s)**

**Please State Reason For Departure(s):**

**Changes and Additions to Specifications:**

4. In addition to the warranties provided in Attachment 1 – Quotation Agreement - Goods, this Quotation includes the following warranties:

5. I/We have reviewed the RFQ Attachment 1 – Quotation Agreement - Goods, Schedule A – Specifications of Goods. If requested by the City, I/we would be prepared to meet those requirements, amended by the following departures (list, if any):

**Section Requested Departure(s) / Alternative(s) / Additions**

**Please State Reason For Departure(s):**

**Fees and Payments (if insufficient space, add additional tables/attachments as required.)**

6. The Contractor shall be responsible for customs clearance and payment of any duties and/or taxes owing at the time of importation into Canada, as applicable. The Contractor offers to supply to the City of Surrey the Goods for the prices plus applicable taxes per below. All duties, handling and transportation charges, and all other incidental charges should be included in the Quotation.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **F.O.B.**  Destination  Freight Prepaid | | **Payment Terms:**  A cash discount of \_\_\_\_% will be allowed if invoices are paid within \_\_\_ days, or the \_\_\_ day of the month following, or net 30 days, on a best effort basis. | | **Ship Via:** |
| **Item** | **Particulars** | | **ONE TONE DUAL REAR WHEEL (DRW) VAN** | **Cost per Unit (CDN $)** |
| 1 | Price per Unit: | | $ |
| 2 | Province of B.C. Environmental Levy (Battery): | |  |
| 3 | Province of B.C. Advance Disposal Fee (Tires): | |  |
| 4 | Air Conditioning Surcharge: | |  |
| 5 | Other Fees/Levies (please state): | | $ |
|  | a.) | |  |
|  | b.) | |  |
|  | c.) | |  |
| 6 | Subtotal: | | $ |
| 7 | GST (5%) on $\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | $ |
| 8 | PST (7%) on $\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | $ |
| 9 | **TOTAL QUOTATION PRICE** | | $ |
| *Pricing is firm until (state date):* | | | | |
| *ALL PRICING IN CANADIAN DOLLARS* | | | | |

**The completed unit shall be delivered within \_\_\_\_\_\_\_ days after receipt of purchase order.**

Year, Make & Model: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Manufacturer’s Warranty: State Warranty

Body Warranty: State Warranty\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Warranty repairs shall be performed at:

Please complete if applicable: British Columbia Certified

**Specifications**

Contractors should complete and submit with their Quotation the Preferred Technical Specifications Response Form. Attach any additional specifications for the Good, any optional accessories and any substitutions for the Good (if substitutions are permitted or applicable).

| **Preferred Technical Specifications Response Form** | **√**  **(Yes)** | **√**  **(No)** | ***Manufacturers’ Specifications of Goods Offered. Contractor should complete all spaces in this column.*** |
| --- | --- | --- | --- |
| 1. **Exterior** | | | |
| 1. Colour – Race Red | □ | □ |  |
| 1. Vans shall have one sliding door on passenger’s side for access to the cargo area. | □ | □ |  |
| 1. Rear doors, side door, and the sides of the van shall have no windows. | □ | □ |  |
| 1. Short arm manual folding, heated power adjusting mirrors external rear vision mirrors. | □ | □ |  |
| 1. Running board for side opening cargo door passengers’ side covers B-C Pillar | □ | □ |  |
| 1. **Axles, Suspension, Chassis** | | | |
| 1. The GVWR should be approximately 11,000lbs. | □ | □ |  |
| 1. Comes with heavy duty trailer hitch package, c/w receiver, hitch to match the maximum towing capability of the vehicle. Includes tow/haul mode. Standard factory trailer wiring to be provided with brake controller. | □ | □ |  |
| 1. Wheelbase should be approximately 148”, overall length approximately 264”. | □ | □ |  |
| 1. Dual rear wheels on rear axle | □ | □ |  |
| 1. All Wheel drive van | □ | □ |  |
| C. Engine - Transmission | | | |
| 1. Engine – Gasoline, provide details | □ | □ |  |
| 1. State engine configuration, size | □ | □ |  |
| 1. Cooling system to -30F | □ | □ |  |
| 1. Automatic transmission – 10 speed W/Overdrive and select shift | □ | □ |  |
| 1. Differential limited slip |  |  |  |
| 1. **Brakes** | | | |
| 1. Brakes should be vacuum/hydraulic type with ABS. | □ | □ |  |
| 1. **Wheels, Tires** | | | |
| 1. Wheels 16” steel, fitted with 205/75R16C winter tires (6) Michelin winter tires preferred (snowflake) | □ | □ |  |
| 1. **Interior** | | | |
| 1. Vehicle interior environment should be fully air-conditioned including a fresh air heater/ventilator/defroster. | □ | □ |  |
| 1. Vehicle should have full flow through ventilation for optimal temperature control and operator comfort. | □ | □ |  |
| 1. Wipers should have intermittent feature. | □ | □ |  |
| 1. Door windows should be power operated. | □ | □ |  |
| 1. Vehicle should include dash mounted power outlet and USB ports | □ | □ |  |
| 1. Vehicle should include AM/FM/ radio with (2) speakers minimum and antenna, with Bluetooth | □ | □ |  |
| 1. Front all weather floor mats | □ | □ |  |
| 1. Vinyl covered front bucket seats. | □ | □ |  |
| 1. Driver and passenger air bags, including side curtain. | □ | □ |  |
| 1. Front overhead shelf | □ | □ |  |
| 1. Large centre console | □ | □ |  |
| 1. Cruise control. | □ | □ |  |
| 1. Full rear compartment lighting, with LED lights | □ | □ |  |
| 1. Heavy duty cargo flooring | □ | □ |  |
| 1. **Electrical** | | | |
| 1. Dual AGM 70 Amp hour each battery | □ | □ |  |
| 1. Upfitter package with high-capacity switches | □ | □ |  |
| 1. Vehicle maintenance monitor | □ | □ |  |
| 1. Auxiliary Fuse Panel | □ | □ |  |
| 1. Reverse sensing system | □ | □ |  |
| 1. Reverse Camera. | □ | □ |  |
| 1. **Miscellaneous** | | | |
| 1. Keyless entry with 3 sets of keys. | □ | □ |  |
| 1. Back up alarm - Grote part # 73040 97 dBA. |  |  |  |
| 1. Fire extinguisher 2.5lb dry powder ABC type. | □ | □ |  |
| 1. WCB Level 1 Basic First Aid Kit | □ | □ |  |
| 1. Front and rear mud flaps. | □ | □ |  |
| 1. The Contractor shall deliver the vehicles, registered, insured, and plated as per the City’s insurance requirements through the City’s insurance broker | □ | □ |  |
| 1. The vehicle shall be rust proofed with a product that provides long term protection and does not require continued reapplication of the product. Contractor to provide details of product offered and warranty. | □ | □ |  |
| 1. **Warranty** | | | |
| 1. Provide details of manufacturer’s warranty | □ | □ |  |
| * One service manual and one parts manual in digital format or CD c/w software * A build sheet shall be provided detailing (but not limited to the following): * VIN * Engine details including serial number * Transmission details including serial number * Diff details including serial number * Oil types and quantities for all components * Tire make, type and size * Engine belts details * Filter list for all components * Battery details * Beacon light make: | □ | □ |  |

7. I/We the undersigned duly authorized representatives of the Contractor, having received and carefully reviewed the RFQ including without limitation the draft Agreement submit this Quotation in response to the RFQ.

**This Quotation** is offered by the Contractor this \_\_\_\_\_\_\_ day of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, 202\_.

**CONTRACTOR**

I/We have the authority to bind the Contractor.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Full Legal Name of Contractor)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Signature of Authorized Signatory)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Print Name and Position of Authorized Signatory)